{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-M"]
[]
[]
[]
[]
["","","","","","FTXM42M2V1B"]
["Opgenomen vermogen","Koelen","","Opgenomen vermogen-=-Koelen-=-Nom.-=-kW (2)","kW","0.035"]
["","Verwarmen","","Nom.","kW","0.035"]
["Behuizing","Kleur","","","","Wit"]
["Afmetingen","Unit","","Hoogte","mm","294"]
["","","","Breedte","mm","811"]
["","","","Diepte","mm","272"]
["Gewicht","Unit","","","kg","10"]
["Ventilator-","Luchthoeveelheid","Koelen","Hoog","m³/min","12.6"]
["Ventilator","Luchthoeveelheid","Koelen","Medium","m³/min","9.5"]
["Ventilator-","Luchthoeveelheid","Koelen","Laag","m³/min","7.1"]
["","","","Fluisterstille werking","m³/min","4.6"]
["","","Verwarmen","Hoog","m³/min","13"]
["Ventilator","Luchthoeveelheid","Verwarmen","Medium","m³/min","10.4"]
["Ventilator-","Luchthoeveelheid","Verwarmen","Laag","m³/min","7.1"]
["","","","Fluisterstille werking","m³/min","5.3"]
["Geluidsvermogenniveau","Koelen","","","dB(A)","60"]
["","Verwarmen","","","dB(A)","60"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dB(A)","45"]
["Geluidsdrukniveau op 1 m","Koelen","","Medium","dB(A)","39"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Laag-=-dB(A)","dB(A)","30"]
["","","","Geluidsdrukniveau op 1 m-=-Koelen-=-Fluisterstille werking-=-dB(A)","dB(A)","21"]
["","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dB(A)","45"]
["Geluidsdrukniveau","Verwarming","","Middelhoog","dB(A)","39"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Laag-=-dB(A)","dB(A)","29"]
["","","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Fluisterstille werking-=-dB(A)","dB(A)","21"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35"]
["Koelleidingmaten","Gas","","Buitendiameter","mm","12.7"]
["Leidingaansluitingen","Drainage","","","","18"]
["Besturingssystemen","Infrared remote control","","","","ARC466A33"]
["","Wired remote control","","","","BRC944B2, BRC073A1"]
["Standaard-accessoires","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Indoor unit fixing screws","","","","2"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["Voeding","Naam","","","","V1"]
["","Fase","","","","1~"]
["Spanningsvorm","Spanningsvorm-=-Frequentie","","Frequentie","","50"]
["","Spanningsvorm-=-Spanning","","Spanning","","220-240"]