{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXG-K"]
[]
[]
[]
[]
["","","","","","FVXG35K2V1B"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.021 (1) (2) (3), 0.021 (1) (2) (3), 0.021 (1) (2) (3)"]
["","Verwarmen","","Nom.","kW","0.024 (1) (2) (3), 0.024 (1) (2) (3), 0.024 (1) (2) (3)"]
["Behuizing","Kleur","","","","Zuiver wit (6.5Y 9.5/0.5)"]
["Afmetingen","Unit","","Hoogte","mm","600"]
["","","","Breedte","mm","950"]
["","","","Diepte","mm","215"]
["Gewicht","Unit","","","kg","22.0"]
["Ventilator-","Luchthoeveelheid","Koelen","Hoog","m³/min","9.1"]
["Ventilator","Luchtdebiet","Koeling","Middelhoog","m³/min","7.2"]
["Ventilator-","Luchthoeveelheid","Koelen","Laag","m³/min","5.3"]
["","","","Fluisterstille werking","m³/min","4.5"]
["","","Verwarmen","Hoog","m³/min","10.2"]
["Ventilator","Luchtdebiet","Verwarming","Middelhoog","m³/min","8.0"]
["Ventilator-","Luchthoeveelheid","Verwarmen","Laag","m³/min","5.8"]
["","","","Fluisterstille werking","m³/min","5.0"]
["Geluidsvermogenniveau","Koelen","","","dB(A)","55"]
["","Verwarmen","","","dB(A)","56"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dB(A)","39"]
["Geluidsdrukniveau","Koeling","","Middelhoog","dB(A)","33"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Laag-=-dB(A)","dB(A)","27"]
["","","","Geluidsdrukniveau op 1 m-=-Koelen-=-Fluisterstille werking-=-dB(A)","dB(A)","24"]
["","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dB(A)","40"]
["Geluidsdrukniveau","Verwarming","","Middelhoog","dB(A)","33"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Laag-=-dB(A)","dB(A)","27"]
["","","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Fluisterstille werking-=-dB(A)","dB(A)","23"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35"]
["","Gas","","Buitendiameter","mm","9.50"]
["","Drainage","","","","18"]
["Besturingssystemen","Infrared remote control","","","","ARC466A2"]
["Standaard-accessoires","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Installation plate","","","","1"]
["","Thermal insulation (thermal insulation tube)","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Drain hose","","","","1"]
["","Remote control holder","","","","1"]
["Voeding","Naam","","","","V1"]
["","Fase","","","","1~"]
["Spanningsvorm","Spanningsvorm-=-Frequentie","","Frequentie","","50"]
["","Spanningsvorm-=-Spanning","","Spanning","","220-240"]
["Opmerkingen","","","","","(1) - 220V"]
["","","","","","(2) - 230V"]
["","","","","","(3) - 240V"]