{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-LV1"]
[]
[]
[]
[]
["","","","","","RZAG71L7V1B"]
["Afmetingen","Unit","","Hoogte","mm","990"]
["","","","Breedte","mm","940"]
["","","","Diepte","mm","320"]
["Gewicht","Unit","","","kg","67"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor"]
["Werkingsbereik","Koelen","","Min.","°C DB","-15"]
["","","","Max.","°C DB","50"]
["","Verwarmen","","Min.","°CWB","-20"]
["","","","Max.","°CWB","15.5"]
["Geluidsvermogenniveau","Koelen","","","dB(A)","64"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Nom.-=-dB(A)","dB(A)","48"]
["","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Nom.-=-dB(A)","dB(A)","50"]
["","Fluisterstille nachtstand","","Geluidsdrukniveau op 1 m-=-Fluisterstille nachtstand-=-Niveau 1-=-dB(A)","dB(A)","43"]
["Koelmiddel","Type","","","","R-32"]
["Koudemiddel","Koudemiddel-=-Inhoud-=-kg","","","kg","2.6"]
["Koudemiddel","GWP","","","","675"]
["Koudemiddel","Vulling","","","tCO2Eq","1.8"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","9.52"]
["Koelleidingmaten","Gas","","Buitendiameter","mm","15.9"]
["Koelleidingmaten","Leidinglengte","","Max.","m","55"]
["","","Systeem","Equivalent","m","75"]
["","","Voorgevuld tot","","m","30"]
["Leidingaansluitingen","Bijkomende koelmiddelvulling","","","kg/m","Zie installatiehandleiding"]
["Koelleidingmaten","Hoogteverschil","","Max.","m","30.0"]
["","","IU - IU","Max.","m","0.5"]
["Standaard-accessoires","Installation manual","","","","1"]
["","Tie-wraps","","","","2"]
["Voeding","Fase","","","","1~"]
["Spanningsvorm","Spanningsvorm-=-Frequentie","","Frequentie","","50/60"]
["","Spanningsvorm-=-Spanning","","Spanning","","220-240"]